From 024dcaaea253e1f69f4325edebec4a9b5618caea Mon Sep 17 00:00:00 2001
From: Martin Mares <mj@ucw.cz>
Date: Wed, 10 Nov 1999 10:48:19 +0000
Subject: Added project status report for KSVI.

---
 doc/status.tex | 90 ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 90 insertions(+)
 create mode 100644 doc/status.tex

(limited to 'doc/status.tex')

diff --git a/doc/status.tex b/doc/status.tex
new file mode 100644
index 0000000..cd7ce89
--- /dev/null
+++ b/doc/status.tex
@@ -0,0 +1,90 @@
+\input mjmac
+
+\hsize=7truein
+\vsize=9.5truein
+\language=\czech
+\chyph
+
+\centerline{\Big Projekt BIRD}
+\bigskip
+\centerline{\Big\ss (Basic Internet Routing Daemon)}
+\bigskip
+\centerline{\large\it zpr�va o~stavu projektu ke~dni 10. 11. 1999}
+
+\vskip 0.5in
+
+\leftline{\Large Obsazen�}
+
+\noindent\halign{\quad \hfil # & \quad # \hfil \cr
+Vedouc� projektu:	& RNDr. Libor Forst \cr
+\noalign{\medskip}
+��astn�ci:		& Ond�ej Filip \cr
+			& Pavel Machek \cr
+			& Martin Mare� \cr
+}
+
+\bigskip
+\leftline{\Large Specifikace}
+
+   C�lem projektu je vyvinout program umo��uj�c� dynamick� routing
+internetovsk�ch protokol� (IPv4 a IPv6) pro opera�n� syst�my kompatibiln�
+s~UNIXem (zejm�na pak pro Linux). Tento program komunikuje s~ostatn�mi
+routery v~s�ti (respektive jej� ��sti, na n�� se dynamick� routing vztahuje)
+prost�ednictv�m standardn�ch protokol� (RIPv2, OSPFv2, BGP4), vym��uje si
+s~nimi informace o~topologii s�t� a jej�ch dynamick�ch zm�n�ch a podle takto
+zji�t�n� topologie nastavuje routovac� tabulky j�dra OS.
+
+   Program d�le zaji��uje distribuci routovac�ch informac� mezi jednotliv�mi
+(jinak na sob� naz�visl�mi) protokoly, p�i�em� tyto informace umo��uje
+filtrovat podle pravidel specifikovan�ch v~jednoduch�m programovac�m
+jazyku, ��m� lze mimo jin� realizovat policy-based routing, kter�
+je jinak dostupn� pouze v~drah�ch komer�n�ch routerech.
+
+   Projekt si rovn� klade za c�l vyu��t nejnov�j��ch vymo�enost�
+modern�ch UNIXov�ch OS, jako jsou v�cen�sobn� routovac� tabulky, netlink
+apod.
+
+   Router bude mo�no za b�hu ovl�dat prost�ednictv�m ��d�c�ch p��kaz�
+p�ed�van�ch po lok�ln�m socketu. To zahrnuje v�pis stavov�ch informac�
+cel�ho syst�mu (routovac�ch tabulek, topologick�ch map protokolu OSPF,
+atributov�ch tabulek BGP a jin�ch �daj� nezbytn�ch pro spr�vce s�t�)
+a zejm�na zm�nu konfigurace bez nutnosti restartu protokol� zm�nami
+nedot�en�ch.
+
+\medskip
+
+\leftline{\Large Stav projektu}
+
+   Po ztr�t� jednoho z~�len� t�mu pokra�uje v�voj pon�kud pomalej��m
+tempem ne� se p�vodn� o�ek�valo, nicm�n� zad�n� projektu hodl�me splnit
+v~cel�m rozsahu a projekt b�hem tohoto �koln�ho roku dokon�it. V~sou�asn�
+dob� chyb� zejm�na dokumentace (jej� nyn�j�� podoba se omezuje v�hradn�
+na~bohat� koment��e ve~zdrojov�ch textech) a podpora protokolu BGP.
+
+\medskip
+
+\noindent Stav jednotliv�ch ��st� projektu:
+
+\medskip
+
+\halign{# \hfil & \qquad \hfil#\cr
+Building system		& 100\%		\cr
+J�dro routeru		& 90\%		\cr
+Spr�va datov�ch struktur & 80\%		\cr
+Podpora IPv4		& 100\%		\cr
+Podpora IPv6		& 70\%		\cr
+Interface na Linux 2.0	& 100\%		\cr
+Interface na Linux 2.2	& 100\%		\cr
+Interface na FreeBSD	& 20\%		\cr
+Protokol RIP		& 90\%		\cr
+Protokol OSPF pro IPv4	& 40\%		\cr
+Protokol OSPF pro IPv6	& 10\%		\cr
+Protokol BGP		& 0\%		\cr
+Interpreter filtr�	& 70\%		\cr
+Parser konfigurace	& 70\%		\cr
+D�lkov� ovl�d�n�	& 20\%		\cr
+Dokumentace		& 0\%		\cr
+Online help		& 0\%		\cr
+}
+
+\bye
-- 
cgit v1.2.3

