From c92795e934758a32472ebc5766ff0f61b1c1409c Mon Sep 17 00:00:00 2001
From: Martin Mares <mj@ucw.cz>
Date: Wed, 31 May 2000 11:28:07 +0000
Subject: Moved old TeX documents to old/ to make them not interfere with doc
 building.

---
 doc/status.tex | 90 ----------------------------------------------------------
 1 file changed, 90 deletions(-)
 delete mode 100644 doc/status.tex

(limited to 'doc/status.tex')

diff --git a/doc/status.tex b/doc/status.tex
deleted file mode 100644
index cd7ce89..0000000
--- a/doc/status.tex
+++ /dev/null
@@ -1,90 +0,0 @@
-\input mjmac
-
-\hsize=7truein
-\vsize=9.5truein
-\language=\czech
-\chyph
-
-\centerline{\Big Projekt BIRD}
-\bigskip
-\centerline{\Big\ss (Basic Internet Routing Daemon)}
-\bigskip
-\centerline{\large\it zpr�va o~stavu projektu ke~dni 10. 11. 1999}
-
-\vskip 0.5in
-
-\leftline{\Large Obsazen�}
-
-\noindent\halign{\quad \hfil # & \quad # \hfil \cr
-Vedouc� projektu:	& RNDr. Libor Forst \cr
-\noalign{\medskip}
-��astn�ci:		& Ond�ej Filip \cr
-			& Pavel Machek \cr
-			& Martin Mare� \cr
-}
-
-\bigskip
-\leftline{\Large Specifikace}
-
-   C�lem projektu je vyvinout program umo��uj�c� dynamick� routing
-internetovsk�ch protokol� (IPv4 a IPv6) pro opera�n� syst�my kompatibiln�
-s~UNIXem (zejm�na pak pro Linux). Tento program komunikuje s~ostatn�mi
-routery v~s�ti (respektive jej� ��sti, na n�� se dynamick� routing vztahuje)
-prost�ednictv�m standardn�ch protokol� (RIPv2, OSPFv2, BGP4), vym��uje si
-s~nimi informace o~topologii s�t� a jej�ch dynamick�ch zm�n�ch a podle takto
-zji�t�n� topologie nastavuje routovac� tabulky j�dra OS.
-
-   Program d�le zaji��uje distribuci routovac�ch informac� mezi jednotliv�mi
-(jinak na sob� naz�visl�mi) protokoly, p�i�em� tyto informace umo��uje
-filtrovat podle pravidel specifikovan�ch v~jednoduch�m programovac�m
-jazyku, ��m� lze mimo jin� realizovat policy-based routing, kter�
-je jinak dostupn� pouze v~drah�ch komer�n�ch routerech.
-
-   Projekt si rovn� klade za c�l vyu��t nejnov�j��ch vymo�enost�
-modern�ch UNIXov�ch OS, jako jsou v�cen�sobn� routovac� tabulky, netlink
-apod.
-
-   Router bude mo�no za b�hu ovl�dat prost�ednictv�m ��d�c�ch p��kaz�
-p�ed�van�ch po lok�ln�m socketu. To zahrnuje v�pis stavov�ch informac�
-cel�ho syst�mu (routovac�ch tabulek, topologick�ch map protokolu OSPF,
-atributov�ch tabulek BGP a jin�ch �daj� nezbytn�ch pro spr�vce s�t�)
-a zejm�na zm�nu konfigurace bez nutnosti restartu protokol� zm�nami
-nedot�en�ch.
-
-\medskip
-
-\leftline{\Large Stav projektu}
-
-   Po ztr�t� jednoho z~�len� t�mu pokra�uje v�voj pon�kud pomalej��m
-tempem ne� se p�vodn� o�ek�valo, nicm�n� zad�n� projektu hodl�me splnit
-v~cel�m rozsahu a projekt b�hem tohoto �koln�ho roku dokon�it. V~sou�asn�
-dob� chyb� zejm�na dokumentace (jej� nyn�j�� podoba se omezuje v�hradn�
-na~bohat� koment��e ve~zdrojov�ch textech) a podpora protokolu BGP.
-
-\medskip
-
-\noindent Stav jednotliv�ch ��st� projektu:
-
-\medskip
-
-\halign{# \hfil & \qquad \hfil#\cr
-Building system		& 100\%		\cr
-J�dro routeru		& 90\%		\cr
-Spr�va datov�ch struktur & 80\%		\cr
-Podpora IPv4		& 100\%		\cr
-Podpora IPv6		& 70\%		\cr
-Interface na Linux 2.0	& 100\%		\cr
-Interface na Linux 2.2	& 100\%		\cr
-Interface na FreeBSD	& 20\%		\cr
-Protokol RIP		& 90\%		\cr
-Protokol OSPF pro IPv4	& 40\%		\cr
-Protokol OSPF pro IPv6	& 10\%		\cr
-Protokol BGP		& 0\%		\cr
-Interpreter filtr�	& 70\%		\cr
-Parser konfigurace	& 70\%		\cr
-D�lkov� ovl�d�n�	& 20\%		\cr
-Dokumentace		& 0\%		\cr
-Online help		& 0\%		\cr
-}
-
-\bye
-- 
cgit v1.2.3

